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	Who’s at Risk?
	Severity
	Likelihood
	Risk Rating
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	Risk Assessment Ratings
	6-9 High Risk
	4 Medium Risk
	1-3 Low Risk

	Key

	A
E = Employees
C = Contractors
P = Public / 3rd parties
	B
3 = Death or Major injury
2 = Reportable  injury
1 = Minor Injury – Time off unlikely
	C
3 = Very likely
2 = Possible
1 = Unlikely or Very Unlikely

	Hazard Control Measures
	Residual Risk

	· A safe system of work is to be in place prior to works being carried out to reduce the risk of the escape of any dust or fumes from the act of removing the lead paint;
· PPE shall be worn. As a minimum head protection, safety boots, safety spectacles, high impact goggles, hearing protection, gloves, respiratory protection and overalls;
· You should ensure that all operatives know how to wear PPE correctly and that they know how to recognise and report PPE failure;
· Ensure any PPE identified in the COSHH assessment is available and worn;
· Local Exhaust Ventilation (LEV) with suitable filters may be utilised where natural ventilation is inadequate;
· All equipment is to be inspected prior to use to ensure that the equipment is not defective. Any defects are to be reported to the Supervisor / Foreman for him to decide on the immediate action required;
· Any equipment supplied is to be maintained and stored in accordance with the manufacturer’s instructions;
· A hot works permit is to be applied for and issued by the Supervisor where Lead Paint is to be removed using a heat gun;
· When removing Lead Paint with a heat gun do not allow the debris to crumble into dust. Damp debris down and place into waste bags;
· Good standards of hygiene are to be adopted both prior to carrying out works and after carrying out works;
· Washing and changing facilities and places free from lead contamination are to be provided where operatives can eat or drink;
· Monitoring of the air is to be carried out to ensure that Occupational Exposure Limits are not exceeded;
· Overalls are to be cleaned on completion of the works and respiratory filters are to be disposed of in accordance with the manufacturer’s guidance.
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