
Seaxe Contract Services Limited		Risk Assessment

	Assessed By:
	Kevin Lovett
	Risk Assessment No:
	RA12

	Hazard Identified:
	Cuts and Injuries from Sharp Objects
	Date Reviewed:
	June 2026

	[image: ]
	A
	B
	C
	D

	
	Who’s at Risk?
	Severity
	Likelihood
	Risk Rating

	
	E
	C
	P
	3
	2
	1
	3
	2
	1
	B x C = D

	
	
	
	
	
	
	
	
	
	
	9

	Risk Assessment Ratings
	6-9 High Risk
	4 Medium Risk
	1-3 Low Risk

	Key

	A
E = Employees
C = Contractors
P = Public / 3rd parties
	B
3 = Death or Major injury
2 = Reportable  injury
1 = Minor Injury – Time off unlikely
	C
3 = Very likely
2 = Possible
1 = Unlikely or Very Unlikely

	Hazard Control Measures
	Residual Risk

	· Suitable hand protection shall be worn at all times unless there is a hazard presented due to loss of dexterity or risk of entanglement in the working parts of machines e.g. drill bits;
· Gloves shall be selected which are suitable for the task and which fit the hand;
· When using saws, knives, etc., hands are to be kept away from the blade at all times and cuts are to be made away from the body;
· Adequate time is to be allocated to undertake work with sharp blades or knives. Do not rush the task as accidents can be the result from being hasty or rushing;
· Do not use excessive force to either free a sharp edge or to try and cut into a dense substance as this often leads to an uncontrolled slip of the blade resulting in an injury to the user;
· Suitable safety gloves are to be worn at all times when moving materials (see also puncture wounds from needle stick injuries);
· Suitable heavy duty gloves and safety glasses must be worn when glass is to be removed in addition to the existing site PPE requirements;
· When undertaking demolition/stripping out activities, suitable heavy duty gloves and safety glasses are to be worn at all times to remove the risk of cuts and injuries from ejected material;
· All cuts and abrasions are to be treated immediately and suitable first aid given. Cuts and abrasions must be covered by waterproof plasters before returning back to work. All accidents/injuries are to be recorded within the site accident book;
· When Stanley knives (or similar) are not in use, blades are to be retracted or stored within a sheath.
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