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	Who’s at Risk?
	Severity
	Likelihood
	Risk Rating
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	C
	P
	3
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	Risk Assessment Ratings
	6-9 High Risk
	4 Medium Risk
	1-3 Low Risk

	Key

	A
E = Employees
C = Contractors
P = Public / 3rd parties
	B
3 = Death or Major injury
2 = Reportable  injury
1 = Minor Injury – Time off unlikely
	C
3 = Very likely
2 = Possible
1 = Unlikely or Very Unlikely

	Hazard Control Measures
	Residual Risk

	· Only trained and competent persons shall carry out a soldering operations;
· Follow all precautions outlined in the Hot Works Permit and ensure that any combustibles are removed or covered;
· Ensure that a suitable fire extinguisher is located at the workplace e.g. water for solid fires, CO2 for electrical fires, dry powder for all fires, foam for fuel/liquid fires;
· Ensure all persons are aware of the emergency procedures for the site;
· Assess the material you are cutting for any potential gases that may be given off.  Specific RPE shall need to be selected and worn;
· Wear the correct PPE, which may require specific eye protection for the risk, flame retardant overalls, gaiters, aprons;
· The area will be checked beforehand to ensure that it is clear of any flammable materials;
· All hot-works will cease 1 hour before the close of work;
· Operatives will carry out a fire check prior to leaving the site;
· During all hot-work operations there will be a portable fire extinguisher to hand;
· Where practicable, all hot-works will be undertaken away from combustible materials;
· Only small quantities of adhesives will be stored on site;
· Adhesive containers will not be exposed to naked flames or extremes of temperature;
· Empty adhesive containers will be disposed of in a suitable container.
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